[Model Supported] DG1022Z,DG1032Z,DG1062Z
[Latest Revision Date] 2017-09-10


[Updated Contents]
v03.01.12.00.00 2017-09-10

- Modified high frequency flatness calibration algorithm


[Previous Versions and Updated Contents]
v00.01.12.00.00	2016-09-29

     - DG1032Z square wave frequency is changed to 25M

v00.01.11.00.00 2016-09-09

- Added a new model DG1022Z

v00.01.10.00.00 2016-08-23

- Added a command for setting the idle level in Burst mode. 
- Resolved the phase deviation problem caused by waveform superimposition. 
- Resolved the problem: During programming, when reading DC waveform offset, 
  the instrument returns Sine waveform offset. 

v00.01.09.00.01 2015-10-30

- Supported seamless interconnection among all RIGOL DS models. 
- Resolved the problems of abnormal LAN communication for a long time 
  and unstable Socket interface. 


v00.01.08.00.00 2015-6-1

- Added the PNG image format and supported reading back and saving the image 
  in PNG format. 
  
- Supported multiple interfaces and updated the LXI, SCPI, and USB Device 
  libraries. 
  
- Added the dual-channel phase synchronization function.

 
v00.01.07.00.02 2014-11-03

- Added the functions of key remote locking and instruction reading 
  via USB disk. 
  
- Added Russian in the system language. 


v00.01.06.00.01 2014-07-25

- Added Traditional Chinese in the system language. 
- Updated LXI underlying driver library to improve the LAN communication speed.
- Resolved the problem: the idle level is not 0 in other modes except Burst.