
#idString UNI-T,UNI-T UT382
#name UNI-T UT382
#handle UT382
#port comfixedbaud
#baudrate 19200
#driver Serial7Seg
#subDriver UT382

#interfaceType Lux
#interface readValue 0

#value Illuminance Lux SI

#notes Hold Menu down to access configuration: press "+ menu menu menu menu menu" to enable USB 

Connector on device is not a standard USB connector, but only works with the supplied cable.
