; This returns the display as a numeric value, the decimal point is controlled by a multiplier

#idString CEM,CEM DT-1309
#name CEM DT-1309
#handle DR1309
#driver DMM2
#subDriver CEMDT1309
#port comfixedbaud
#baudrate 9600

#readingDelay 1

#interfaceType Lux
#interface readValue 0

