
#idString Peaktech,Peaktech 2025A,
#name Peaktech 2025A
#handle P2025
#port comfixedbaud
#baudrate 9600
#help SimpleDMM
#driver DMM2
#subDriver Peaktech2025A

#readingDelay 1


#interfaceType DMM
#interface readValue 0

#notes Ensure that "RS232" on the Peaktech 2025A is off when "TestController" is trying to detect the meter for the first time.

Remember to disable Auto Power Off (APO) for long term logging: press and hold SELECT while switching the meter on. Meter will beep after 15 minutes and several times thereafter indicating that APO is off.